 Run initial\_file.m to convert to .mat-file and ascii-file. Then use read\_data\_dcd\_modified.m to convert ascii to dcd. Double check that that the channels are correct to your measurement data and set offset etc.  
  
You might want to use some Matlab filter to filter the data. The steering wheel angle is filtered by a simple filter at the end of the initial\_file.m